**Appendix G - Wheelchair Check Form**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Team** | **Team representative** | **Athlete number** | A check resulting in a Pass should be marked with a P. Leave blank if the chair fails the check |
|  |  |  |
| **Athletes name** |  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  | **IWRF International Rules; section 4** | **Comments or Not Applicable**  | **Pass** | **Fail** |
| **Length** | From rear wheel: 46cm |  |  |  |
| **Bumper** | Maximum height: 20cm |  |  |  |
|  | First point of contact: 11cm (+/– 5mm) |  |  |  |
|  | Minimum 3cm off the floor |  |  |  |
|  | Maximum length: 20cm |  |  |  |
|  | Minimum width at first point of contact: 20cm |  |  |  |
|  | Maximum 2cm outside caster housing |  |  |  |
|  | 45° angle or greater |  |  |  |
| **Wings** | First point of contact: 11cm (+/– 1cm) |  |  |  |
|  | Maximum height: 20cm |  |  |  |
|  | Minimum 3cm off the floor |  |  |  |
|  | Obstacle-free space is clear |  |  |  |
|  | Centre of tire or further in |  |  |  |
| **Ball Holder** | Rigid and a minimum of 19mm diameter |  |  |  |
|  | Well padded and permanently fixed to the frame (brackets for removability are permitted) |  |  |  |
|  | Device partially supports the ball while the athlete is in a neutral position |  |  |  |
|  | No part of the ball rests within frame |  |  |  |
|  | 75% of ball is visible above the ball holder |  |  |  |
|  | No mechanical advantage (adhesive free, etc.)  |  |  |  |
|  | Closed shape device - 14cm or less between the widest 2 points (inside measurement) |  |  |  |
|  | Additional ball holders are checked and legal |  |  |  |
| **Rear bar** | Only one brace bar, well padded |  |  |  |
| **Anti-tip** | 2 anti-tip devices minimum 40cm apart |  |  |  |
| **Other** | Rear wheel contact with wall |  |  |  |
| If applicable | No Adhesive (Casters, Tires, Spoke Guards) |  |  |  |
|  |  |  |  |  |
| Clothing & Numbers (Art. 21) | Shirt number – front left side (10 cm) |  |
|  | Shirt number - back center (between 12 and 20 cm) |  |
| Hand protection (Art 22.) | Checked |  |
|  |  |  |
| Uniform Colours (2 contrasting colours) |  |  |  |  |
|  |
| Competition Regulations – IWRF Interim Uniform Policy (see below)  |  |  |
| Uniform sponsorship logos must be grouped in the centre of the shirt (front & back – back includes sleeve space) each grouping must not exceed 160 cm2 (including sleeves). In addition to the manufacturer’s logo Uniform manufacturer logo max 30 cm2.  |
| No sponsor marks are permitted on gloves, shoes, sleeves or headgear. Manufacturing mark on padded head gear 10cm2  |
| No sponsor marks are permitted on the back of the chair or on the frame, other than the manufacturers logo as commercially available (The IWRF or LOC reserves the right to use this space)  |
| Competition spoke guards may have a sponsor logo space of 160 cm2. Sponsor logos on all competition wheels must look the same (including wheels on the bench)  |
| Comments: |
|  |
|  |
|  **Form completed & verified by IWRF** |  **Sign off when chair is legal**  |
| Name |  |  Signature |  |
| IWRF Role |  |  Date |  |
|  **Form acknowledged by team representative**  |  |  |  |
| Name |  |  Signature |  |
|  |  |  Date |  |